# Royal Victoria Collection — BIM & CAD Material Library
## Version 1.2 | August 2026

**Website:** royalvictoriacollection.com.au  
**Phone:** 0488 410 827  
**Showrooms:** Rocklea, Arundel, Archerfield, Brendale QLD | Chinderah NSW

---

## What's in this package

```
RVC-BIM-Package/
├── RVC_Stone_Materials.adsklib     ← Revit/Autodesk material library (import directly)
├── Textures/                       ← Stone texture images
│   └── RVC_[ColourName]_2K.jpg     ← Texture image for renders (target 2048px wide)
├── SketchUp_Materials/             ← SketchUp material XML definitions
└── README.md                       ← This file
```

---

## How to use in Revit

1. Open Revit
2. Go to **Manage** tab → **Materials**
3. In the Material Browser, click the **Open Existing Library** icon (📂)
4. Navigate to and select **RVC_Stone_Materials.adsklib**
5. All 48 RVC stone colours will appear in your material library
6. Drag any material onto a surface, or assign via the material properties
7. In the Appearance tab, the texture image is already linked — ensure the **Textures/** folder stays in the same directory as the .adsklib file

**Tip:** For best render results, set the material scale to 3200mm × 1600mm (actual slab size).

---

## How to use textures in other software

### 3ds Max / V-Ray / Corona
1. Create a new material
2. In the Diffuse channel, load the texture from the **Textures/** folder
3. Set tiling to 1×1 (non-repeating) for realistic slab representation
4. Glossiness: 0.85 | Reflection: 0.1 | Bump: minimal

### ArchiCAD
1. Go to **Options** → **Element Attributes** → **Surfaces**
2. Create new surface, load texture from Textures/ folder
3. Set size to 3200mm × 1600mm

### Enscape / Lumion
Load the 2K texture files (RVC_[Name]_2K.jpg) for optimal performance.

### SketchUp
Import the XML files from **SketchUp_Materials/** folder, or manually create materials using the texture images.

---

## Product Information

| Property | Detail |
|----------|--------|
| Slab size | 3200mm × 1600mm |
| Thickness | 20mm or 30mm (30mm available in all colours — unique to RVC) |
| Finish | Polished standard |
| Silica content | <1% — compliant with Australian silica regulations |
| Warranty | Available on request |

**Note:** RVC is the only brand in Australia offering 30mm thickness across the full colour range.

---

## Colours in this library

- Amalfi *(not in current core range — legacy/limited name, confirm before specifying)*
- Amazonia
- Amethyst
- Aurelia
- Avorio
- Bolivia Blue
- Brazil
- Brazilian Gold
- Breche
- Calacatta Viola
- Copper Sunset
- Cremant
- Cristallo Rose
- Dune
- Dune - Dark
- Emerald Mist
- Espirato
- Essence
- Florence
- Frost White *(not in current core range — legacy/limited name, confirm before specifying)*
- Fusion Green
- Gallant Grey *(not in current core range — legacy/limited name, confirm before specifying)*
- Grand Calacatta
- Green Onyx
- Jardin Marble
- Julius
- Lush Carrara
- Mint Onyx
- Montebello
- Mythical Grey *(not in current core range — legacy/limited name, confirm before specifying)*
- Panda Grey
- Panda White
- Pearl Ivory
- Phantom Jade
- Pink Onyx
- Princess White
- Raindrops *(not in current core range — legacy/limited name, confirm before specifying)*
- Sienna Gold
- Silky White *(not in current core range — legacy/limited name, confirm before specifying)*
- Statuaria Gold
- Super White Dolomite *(limited release — confirm current availability)*
- Taj Ivory
- Taj Mahal - Classic
- Taj Mahal - Light
- Taj Mahal - Warm Beige
- Thunderstorm
- Tuscany Marble *(pending — source image not yet available, not included in this package)*
- Viola Burgundy
- White Onyx

---

## Contact & Samples

Physical samples available from all showroom locations.  
For project specifications and pricing: **royalvictoriacollection.com.au** or call **0488 410 827**

*© 2026 Royal Victoria Collection. All images are representative of the stone surface. Natural variation exists between slabs.*
